To initiate the modelling, the computational mesh is constructed to
cover the available data. The resolution is chosen to balance
computational time and desired resolution in areas of interest,
particularly in the interface between the on and offshore. The
following series of figures illustrate the study extent for the
scenario and the resulting computational mesh, highlighting areas
of refinement around areas of particular interest.


\begin{figure}[hbt]

  %\centerline{ \includegraphics[width=75mm, height=75mm]{figures/.eps}}

  \caption{Study area for Pt Hedland scenario}
  \label{fig:pt_hedland_area}
\end{figure}


\begin{figure}[hbt]

  %\centerline{ \includegraphics[width=75mm, height=75mm]{figures/.eps}}

  \caption{Computational mesh for Pt Hedland study area}
  \label{fig:mesh_pthedland}
\end{figure}
